TECHNICAL SPECIFICATIONS 				SECURITY SYSTEM
DIVISION 13 - SPECIAL CONSTRUCTION
SECTION 137_ _ - SECURITY CCTV SYSTEM

PART 2 - PRODUCTS
2.01 GENERAL
A. All equipment and materials used shall be standard components, regularly 
manufactured, regularly utilized in the manufacturer’s system.
B. All systems and components shall have been thoroughly tested and proven in actual 
use.
C. All systems and components shall be provided with the availability of a toll free 24-
hour technical support phone number from the manufacturer. The phone number shall 
allow for immediate technical assistance for either the dealer/installer or the end user at 
no charge.
D. All systems and components shall be provided with an explicit manufacturer warranty.

2.02 (Vicon model SVFT-WM) WALL MOUNT
A. The wall mount shall allow pendant installations of particular proprietary camera dome 
systems.
B. The wall mount shall be usable in indoor and outdoor applications.
C. The wall mount shall allow mounting on a wall or vertical structure.
D. The wall mount shall have a standard 1-1/2 in. NPT-F pipe thread.
E. The wall mount shall have the following mechanical specifications:
1. Mounting: Wall or vertical structure.
2. Dimensions: Height: 4.9-in. (124 mm).
Width: 3.5-in. (89 mm).
Depth: 7.5-in. (191 mm).
3. Weight: 1.4-lb (0.6 kg).
4. Construction: Cast aluminum, steel and stainless steel.
5. Color: White.

The Wall Mount shall be Vicon Industries model number SVFT-WM.

Spec V141-00-00